**Memory Map for the LFSR**

Reg map;

\* 00: read LFSR out

\* 01: control register

wr\_data(0) : init (load hardcoded initial value to the registers)